EESchema-DOCLIB  Version 2.0  Date: 21/08/2012 10:54:45
#
$CMP 74HCT138
D Decoder 3 to 8 (active low outputs)
K TTL DECOD DECOD8
$ENDCMP
#
$CMP 74HCT245
D Octal BUS Transceivers, 3 State out
K TTL BUS 3State
$ENDCMP
#
$CMP 74HCT32
D Quad Or 2 inputs
K TTL Or2
$ENDCMP
#
$CMP FT245RL
D FT245RL
K FTDI USB FIFO
$ENDCMP
#
$CMP SST39SF010A
D 1 Mbit Multi-Purpose Flash
K 128KB flash
$ENDCMP
#
#End Doc Library
