Q: Why is there so many .bin files ??
A: In order to use SatCom FirmWare's features in several conditions
   of use, 3 different output files are created :

 1. Use from CD-R: SatCom Live CD
     This is the recommended way of testing SatCom features.
     Simply burn SCFirmWare.iso to a CD-R, then run it from your Saturn.
     You may need to perform the swap trick, or use a modchip.

     Path: SCFirmWare/release/SCFirmWare.iso


 2. Use by uploading to your Saturn: SatCom Program.
     In the case you can't use CD-R, you can upload SatCom Program file
     to your Saturn (execute address is 0x06004000).
     Example when using USB Data Link:
      1) Upload and execute SatCom Program by using USB Data Link's original software.
      2A) Upload other data by using SatCom software, and enjoy fast transfer rate
          thanks to SatCom data compression support for USB Data Link !
      2B) Flash your ARP's firmware directly from your PC by using SatCom debugger !

     Path: SCFirmWare/release/SCProgram.bin


 3. Use from your ARP: SatCom FirmWare.
     If testing SatCom FirmWare succeded, you should install it on your ARP
     over its original firmware.
     To perform this, simply follow the flashing instructions in SatCom Live CD.
     IMPORTANT: By flashing your ARP, its firmware, and backup data
                you saved from ARP's menu will be erased !!!
                You should backup your ARP's flash memory before flashing it !

     Path: SCFirmWare/cd/ARP/firm.bin



Q: Can I flash my ARP without burning CD-R ?
A: Yeah, it is possible !
   If you could upload SatCom Program to your Saturn, let's use SatCom debugger's
   file I/O feature in order to send the firmware data to your Saturn.
   A) Open SatCom debugger (SatLink.exe), and open/test connection with your Saturn.
   B) In "Misc. Settings" tab, set "Read/Write folder" to "SCFirmWare\cd", and push "Set" button.
   C) In "Debugger" tab, check "Use Debugger" checkbox.
      If debugger status in the status bar is updated, and if no error message is
      displayed in the log area, it should be OK.
   D) From SatCom Program's ARP flash menu, select "SatCom firmware by cafe-alpha (PC)".
       -> SCFirmWare\cd\ARP\firm.bin will be sent to your Saturn, then flashed to your ARP.



Q: How can I flash back my ARP to its original firmware ?
A: A) As some ARP original firmwares are included in SatCom Live CD, you simply need to
      select a firmware from the SatCom Live CD's ARP flash menu.
   B) When using SatCom Program, simply overwrite ARP/firm.bin file with the firmware
      of your choice, and perform the procedure explained in the previous question.



